CV620-BI/WI FW VCBF109 Notes:
1. To modify the “Initial Position” control command to be consistent to other models.
 	
Initial Position:
Command
8x 01 04 75 6A 0p FF
Reply
NA
 
Initial Position Inquiry:
Command
8x 09 04 75 6A FF
Reply
y0 50 0p FF
 
Before
p:
2: Preset 0
3: Last Memory
 
After
p:
1: Preset 0
0: Last Memory