Firmware Notes:

1. You will need an empty thumb drive no larger than 16GB (Larger thumb drives will not work)
2. The drive will need to be FAT32 formatted from your computer.
3. Drop the unzipped RCP firmware file onto the drive.
4. Power on your CV-RCP-V2 unit.  
5. Then insert the Thumb Drive into the USB slot on the back of the unit.
6. The RCP will prompt you to update and will load in a few seconds.
7. To confirm look on the bottom right-hand corner of the screen and you should see the new firmware number. 


